Win2000 AGP driver 

for SiS 5591 / 600 / 530 / 620 / 540 / 630

To install this driver: 
1. Go to device manager, right-click on the PCI-PCI bridge 
   which represents your AGP bridge and select "Properties". 
2. Select the "Driver" page and push the "Update Driver" 
   button. Go through the update driver wizard and on the 
   "Locate Driver Files" page select "Specify a location"
3. Enter the location of your new INF and driver.
