    SiS IDE Driver Installation For Windows 95
    ==========================================
1. Please put SiS IDE Drivers diskette in Floppy drive or
   CD-ROM drive.

2. Please run the file "setup.exe" under "Win95" directory
   in SiS IDE Drivers diskette and follow the instructions
   to install the SiS IDE Windows 95 PIO/DMA Drivers.

Notice:

   Under Windows 95, system will hang when accessing IDE 
   CD-ROM Driver motion happened, such as open "My Computer", 
   CD-ROM Autoplay ...... etc.

   When this situation happened, 
   SiS suggest remove IDE CD-ROM DOS Driver provided by device 
   company.

   IDE CD-ROM DOS Driver Removing Procedure:

   1. Remark or delete "mscdex.exe"  command in c:\autoexec.bat.
   2. Remark or delete IDE CD-ROM DOS Driver in c:\config.sys.