SiS 5503 Compliant South Bridge PCI IRQ Routing Miniport Driver
Installation Guide
===============================================================

[Requirement]

(1) SiS SISPCIMP.PCI
    This VxD only supports SiS 5503,5513,5571,5598,5595 chipset.

(2) Win95 OSR2.1
    You need use Usbsupp.exe from Microsoft to upgrade Win95 OSR2 to OSR2.1.
    In order to make sure your system is running on OSR2.1, find the subkey
    "HKEY_LOCAL_MACHINE\SOFTWARE\Microsoft\Windows\CurrentVersion", and see
    if the value of "VersionNumber" is either "4.03.1212" or "4.03.1214".


Installation Instructions
=========================
(1) Run program "SETUP.EXE" in the SiS PCI IRQ Miniport driver floppy and it
    will install the miniport Driver automatically onto your Windows 95 system.

Update Note
===========
Version1.1
Remove "Forced IRQ 7Xh" Problem

