ESS SOLO-1 PCI audio NT4.0 Drivers Note
-------------------------------------------------

* For Windows NT 4.0 drivers installation
  1. Press "Start" button.
  2. Move highlight bar to "Settings" and select "Control Panel".
  3. Double click on "Multimedia" icon.
  4. Select "Devices" page.
  5. Press "Add..." button.
  6. Select item "Unlisted or Updated Driver" in "List of Drivers" list box.
  7. Specfy path of PCI audio NT drivers.(EXAMPLE CD PATH : F:\ESSOLO-1\WNT40)
  8. The dialog show item that fit your audio device, please press "OK" button.
  9. Choose proper I/O or "OK" button for default setting.
 10. Please restat Windows NT system.

* How to remove installed drivers?
  1. Press "Start" button.
  2. Move highlight bar to "Settings" and select "Control Panel".
  3. Double click on "Multimedia" icon.
  4. Select "Devices" page.
  5. Open "Audio Devices".
  6. Select "Audio for C-Media PCI Devices" then press "Remove" button.
  7. Press "Yes" button while system ask for confirming.
  8. Shut down NT system and reboot.