
Test Plan

Function Name:
    South Bridge PCI IRQ Routing Miniport Driver

Hardware requirement:
    SiS 5503/5513/5571/5598/5595 chipset

Software requirement:
    Windows 95 OSR2.1
    Make sure the subkey "HKEY_LOCAL_MACHINE\SOFTWARE\Microsoft\Windows\CurrentVersion"
    should be equal to either "4.03.1212" or "4.03.1214"

Installation:
    Run program "setup.exe" in the driver floppy disk and it will install the
    miniport driver automatically.

Test procedure:
    Reboot the computer after the installation is completed succeddfully.
    Make sure the following requirements are met.
    1. IRQ steering is enabled. Check the path:
       Control Panel -> System -> Device Manager -> System Devices ->
       PCI bus -> IRQ Steering, there is a group box labeled "IRQ status",
       which shold show you that the IRQ steering is enabled.
    2. IRQs are properly assigned. Check the path:
       Control Panel -> System -> Device Manager, double click the computer
       icon, a list of IRQ resources would be given.
    3. Please use HCT 7.6 test package. Check the system/bus/pci item.

